**Venetian blind motor GJ56.. AIR**

**Motor**

230V / 50Hz motor for concealed installation, torque: 6, 10, 16 or 20 Nm,

speed: 26 r / min, protection class IP 54, with integrated, multi-stage planetary gear and two-sided shaft, built-in limit stop switch, capacitor and thermal overload protector. Pluggable connection cable. The motor is permanently lubricated and maintenance-free.

Several motors can be connected in parallel. Integrated bidirectional radio module AIR.

The motor must be installed with a noise-optimized damping to reduce the borne sound transmission to a minimum.

Upper and lower limit stops are freely adjustable, even without standard setting switch. The shutdown in the upper end position can be carried out by means of the limit stop switch without any further setting. With antifreeze protection and length adjustment of the blind via automatic referencing after 1, 5, 20 and then every 50 cycles. Compatible with LOXONE Smart Home control.