**GJ56..E07 SMI - Motor for Venetian blinds**

**Motor**

230V / 50Hz motor for concealed installation, torque: 6, 10, 16 or 20 Nm according to type,

speed: 26 r / min, IP 54, with integrated, multi-stage planetary gear and two-sided shaft, built-in limit stop switch, capacitor and thermal overload protector. Pluggable connection cable. The motor is permanently lubricated and maintenance-free.

Several motors can be connected in parallel.

The motor must be installed with a noise-optimized damping to reduce the borne sound transmission to a minimum.

Upper and lower limit stops are freely adjustable, even without standard setting switch. Optional shutdown in the upper end position by means of the limit stop switch without any further setting.

With antifreeze protection and length adjustment of the blind via automatic referencing after 1, 5, 20 and then every 50 cycles.

Compatible with SMI automation systems and SMI for Venetian blind systems with automatic solar tracking. Parallel connection and individual control of max. 16 SMI motors with SMI actuator.