**SOLIDline Flex AIR – Smart Home Ready**

**Motor**

230V / 50Hz electronic tubular motor for concealed installation, torque: 10, 20, 30, 40,

50 Nm according to type, speed: 16 r / min (with 50 Nm 12 r/min), IP 44, with integrated, multi-stage planetary gear, mounted capacitor and thermal overload protector. Pluggable connection cable. The motor is permanently lubricated and maintenance-free. Several motors can be connected in parallel. Integrated bidirectional radio module AIR.

**Application**: rolling shutters (with or without stops/ anti-lift device), screens (ZIP screens, facade awnings etc.), open style folding arm awnings.

The setting of the upper and lower end positions can be carried out via a torque-controlled shut-off or via freely adjustable positions. Compatible with the LOXONE Smart Home control system.