**SOLIDline ZIP AIR – Smart Home Ready**

**Motor**

230V / 50Hz electronic tubular motor for concealed installation, torque: 6, 10, 20, 30 Nm according to type, speed: 16 r/min, IP 44, with integrated, multi-stage planetary gear, mounted capacitor and thermal overload protector. Pluggable connection cable. The motor is permanently lubricated and maintenance-free. Several motors can be connected in parallel. Integrated bidirectional radio module AIR.

**Application**: screens with ZIP guidance

The setting of the upper and lower end positions can be carried out via a torque-controlled shut-off or via freely adjustable positions. Compatible with the LOXONE Smart Home control system.