# Zhaoxin® Universal Inter-Integrated Circuit (I2C) Windows Software Package Release Notes

2024-01-12

Support Platforms

Component version inside this package

Notices

Installation and Remove

Known Issues

Limitations

Revision History

DISCLAIMER

# Support Platforms

## Hardware:

u This package supports the following chips:

Ø KX-6000G

Ø KX-7000

u Hardware Device ID table:

Chipset | Device ID
KX-6000G | ACPI\IIC1D17
KX-7000 | ACPI\IIC1D17

u Other chips supported are not guaranteed.

## Operating System:

This software package only supports Microsoft Windows© Platforms. The setup program will detect the current platform and install proper driver on your system. The supported platforms are list below:

u Windows NT x64-bits Platform

Ø Windows 10

Ø Windows 11

u Windows NT X86-bits Platform

Ø Windows 10

Back to top

# Component version inside this package

Component | Name | Version
ZX I2C driver | ZXSPBI2C.inf/sys | V1.10B

Back to top

# Notices

1. BIOS reside in the motherboard must enable the I2C Host Controller.

2. For KX-XXXX platform, the touchpad device must to connect to KX-XXXX platform. The following are supported touchpad brands

a. Goodix GXTP7863

3. When you are ready to test your driver in Static Tools Logo Test using the Windows Hardware Lab Kit on Win11, you need to copy the driver verification log (DVL) to the C:\DVL directory on the test computer. Be sure to delete the contents of the directory on the test computer before you copy the new driver verification log.

4. If you wish to select another touchpad device, please ask BIOS developer to modify device address on ACPI table and programming the modified firmware BIOS into the platform.

Back to top

# Installation and Remove

## Installation

1. Unzip Zhaoxin Universal I2C indows Software Package, then open Zhaoxin Universal I2C Windows Software Package folder.

2. Run SETUP.EXE.

3. Select modules to be installed, then click “next” until the setup process is completed.

4. Reboot OS.

## Remove

1. Open the “Add/Remove Program” in Control Center

2. Click the Add/Remove button to remove Zhaoxin I2C Windows Controller Driver.

Back to top

# Features

1. Goodix GXTP7863 touchpad feature

è Support precision touchpad (PTP).

è Reference : https://support.microsoft.com/en-us/windows/touch-gestures-for-windows-a9d28305-4818-a5df-4e2b-e5590f850741

suBack to top

# Known Issues

Back to top

# Limitations

Back to top

# Revision History

Version | Release Date | Comments
Version 1.10B | 2024/01/12 | This version : 1. Support Windows 10 X86 Microsoft certification
Version 1.10A | 2024/01/03 | This version : 1. Support Microsoft certification 2. Support KX-6000G & KX7000 platform
Version 1.00A | 2023/05/12 | First initial version : Only Support KX-6000G platform

# DISCLAIMER

Information in this document is provided in connection with Zhaoxin Universal I2C software packages. Shanghai Zhaoxin Semiconductor Co., Ltd assumes no responsibility for any errors in this document. Any part of document MUST NOT be reproduced, transmitted, or translated into any language, or in any form without the prior written permission of Shanghai Zhaoxin Semiconductor Co., Ltd

Zhaoxin may make changes to specifications and product descriptions at any time, without notice.

Copyright © 2015 Shanghai Zhaoxin Semiconductor Co., Ltd

Back to top

All copyrights are reserved by Shanghai Zhaoxin Semiconductor Co., Ltd http://www.zhaoxin.com