
**Circular tube horizontal scraping linkage**


It is suitable for bus models with wide body ,and can be designed and matched according to the front size or three-dimensional data provided by customers.






**Horizontal channel scraping linkage**


It is suitable for bus models with wide body ,and can be designed and matched according to the front size or three-dimensional data provided by customers.






**Channel steel vertical double linkage**


Suitable for buses with two front








**Channel steel along scraping linkage**

Suitable for minibuses, heavy trucks and other narrow commercial vehicles







**Single wiper arm linkage**




**Double rod scraper arm linkage**





**A0 plan linkage and de motor assembly**

Applicable vehicle model: Shandeka



**C7 Wiper linkage and motor assembly**

Applicable vehicle model: Shadeka

